Safe Work Method Statement
	Business
	

	ABN
	

	Job / task
	

	Work date
	

	Site
	

	Prepared by
	

	Responsible
	


High Risk Construction Work: tick every category this work involves
☐  Risk of a fall more than 2 metres
☐  Work on a telecommunication tower
☐  Demolition of a load-bearing element
☐  Likely disturbance of asbestos
☐  Structural alteration requiring temporary support
☐  Work in or near a confined space
☐  Excavation, shaft or trench deeper than 1.5 metres
☐  Work in a tunnel
☐  Use of explosives
☐  Work near pressurised gas mains or piping
☐  Work near chemical, fuel or refrigerant lines
☐  Work near energised electrical installations
☐  Work in a contaminated or flammable atmosphere
☐  Tilt-up or precast concrete
☐  Work on or near a road, railway or traffic corridor
☐  Work in an area with movement of powered mobile plant
☐  Work in artificial extremes of temperature
☐  Work in or near water with a risk of drowning
Hazards, risks and control measures
	Hazard
	Risk
	Control measures
	Residual risk (before / after)

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	


How controls are monitored and reviewed
The supervisor checks all listed controls are in place before work starts and monitors them throughout the job. Work stops and this SWMS is reviewed if conditions change, a new hazard appears, or after any incident or near miss.
Crew acknowledgement and signatures
By signing, each crew member confirms this SWMS was explained to them and they will follow it.
	Name
	Role
	Signature
	Date

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	


Free SWMS template from chippieapp.com/swms-app, where Chippie builds this document from a trade hazard library and takes crew signatures on site.




